Headless Headunit

# Connections

* 24V power to car battery
* Left, Right channels to speakers
* Antenna
* Control cable to control box

# Powering up

Power up the unit by flipping the power switch.

The unit will continue playing where it left off when powering down, as long as that source is still available.

After uploading files to the Samba share, push the bottom button to update the local database and start playing.

# Remote control

Buttons:

|  |  |
| --- | --- |
| Button | Function |
|  |  |
| Source | Jump to next source:  Bluetooth → Previously playing source  FM → USB*1* → USB*2* → USB*n* → SD card → Line in → FM |
| Random | Plays random track  Only available for: USB, SD  Setting is not stored (?) *should we?* |
|  |  |
|  |  |
|  |  |
|  |  |

# Sources

|  |  |
| --- | --- |
| Source | .. |
| FM | Radio |
| USB | Flash drive |
| SD card | Internal storage |
| Line-in |  |
| Bluetooth | Start playback by pairing your phone or other Bluetooth device, and starting playback. Cannot be selected through [SOURCE] |

x